SOFTWARE 2014 CHECKLIST

* Check pneumatics defaults
* Check drives encoders
* Check ball sensor (True = don’t see ball, False = see ball)
* Check upper/lower limit switch (True = no touch, False = touch)
* Pivot motor (Positive = up, Negative = down)
* Check pivot encoder
* Check winch pot (Less than 0.5 volts)
* Winch motor (Positive = unwinds, Negative = winds)
* Check latch switch (True = untouched, False = touched)
* Acq motor (positive = acquire, Negative = eject)